**Specification**

**Date:** 1/9/24

**Project Name:** Tactile On/Off Switch Button

**Responsible:** D. Shlenkevitch

**Electrical:**

Input/Output Voltage: 0 – 12 V

Current: < 2 A

Input/Output: Screw Terminal

Power available indicator: Green LED

**Mechanical:**

Height: < 20 mm

Length: < 20 mm

Width: < 40 mm (Flexible)

Mounting side: panel outer side

Optional: PCB with mounting holes for mounting on inner side

**Software:**

N/A